{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Attachment VI Link Connectivity"],"not_rendered":{"images":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Attachment VI Link Connectivity","index":0,"n_rows":20,"n_cols":4,"rows_kept":20,"merged":[[1,0,1,3],[4,0,4,3],[7,1,7,3],[8,1,8,3],[12,0,12,3],[15,0,15,3],[16,0,17,1],[18,0,18,3],[19,0,19,3]],"flags":["formulas_cached_only"]}
[]
["Annex 1.6\n    CFFEX Circuit Connectivity Test Report"]
[null,null,"No."]
[]
["Basic Information of Member"]
["Company Name",null,"Date"]
["Short Name",null,"Member ID"]
["Contact Address"]
["Member-end Access Address"]
["Technical Contact Person",null,"Contact Phone"]
["Mobile Phone",null,"Fax No."]
["E-mail",null,"Post Code"]
["Circuit Information"]
["Access Method",null,"Bandwidth"]
["WAN IP",null,"LAN IP:"]
["Circuit Connectivity Test"]
["WAN IP of Router of PING Exchange-end",null,"Packet Loss Rate:","Min. Delay:"]
[null,null,"Average Delay:","Max. Delay:"]
["We have completed the circuit connectivity test and relevant performances have been able to meet the service requirements.                                                 "]
["Remarks: \n1. It is prohibited to test it during the trading period. The test may be arranged on a non-trading day or after 16:30 on a trading day;\n2. The source address of test packages is WAN interface ip of member-end, and the target address is WAN  interface ip of Exchange-end;\n3. It is forbidden to ping trading front or mdfront;\n4. PING 10,000  1,500-byte packets;\n"]